Translate This

- Pet
  Strapping
- Pet Strapping
  Tools
- PP Multi
  Filaments Yarn
- PP Crimp
  Yarn
- High Tenacity
  Twine
- PP Filler Cord
  / Dust Proof

- ### Welcome to Straps India

  Straps India is a leading manufacturer of plastic products in India with world best production technologies. Company occupies an enviable position in the domestic as well as international market with its wide range of PP and HDPE and PET products. Company is well known for their best service and quality products. Company's group turnover is nearly USD 20 MILLION in financial year 2011-12.

  Company is in plastic business since last 20 years. Installed capacity of company is nearly 8000MT per year. Company is the largest manufacturer of PP multi filament yarn, twine, tapes, ropes and fishing nets, sports net, agricultural nets.

  ### Infrastructure

  - SML Austria for MFR of high tenacity PP multi filament yarn.
  - WITIN USA for MFR pf high tenacity twine and thread.
  - KOREAN technology for MFR of all kind of nets and rope business.
  - Reimotec gmbh Germany (Reifenhauser gmbh group) for mfr. of pet strap.
  - KY looms Taiwan for narrow woven fabrics and webbing.

  ### Our Products

  ##### Pet Strapping

  ##### Pet Strapping Tools

  ##### PP Multi Filaments Yarn

  ##### PP Crimp Yarn

  ##### High Tenacity Twine

  ##### PP Ropes

- ### category

  - Pet Strapping
  - Pet Strapping Tools
  - PP Multi Filaments Yarn
  - PP Crimp Yarn
  - High Tenacity Twine
  - PP Ropes

  ### product overview

  #### Pet Strapping

  Straps India is having world best twin screw extrusion line from Reimotec gmbh Germany for pet strap production.

  READ MORE

  #### Pet Strapping Tools

  Company provides full range of pneumatic and battery operated pet strapping tools made by M J Maillis.

  READ MORE

  #### PP Multi Filaments Yarn

  Company provides high tenacity PP multi filament yarn produced with world best extrusion line of SML Austria.

  READ MORE

  #### PP Crimp Yarn

  Company owns JSW extrusion line with TEIJIN SEIKI winders for production of PP crimping yarn.

  READ MORE

  #### High Tenacity Twine

  We MFR all types of two and multiple plied twine commonly used as stitching and sewing thread for bags in sugar, rice and fertilizer industry.

  READ MORE

  #### PP Ropes

  We are having Korean extrusion line for production of PP Danline Ropes.

  READ MORE

- ### careers

- ### Company provides pet strapping for following industries

  - Cotton Baling.
  - Fibre Baling.
  - Poly Packet Packing.
  - Tiles & Paver Block Packing.
  - Timber & Wood Packing.
  - Alluminium Ingot Packing.
  - All Kind Of Film Packing.
  - Glass Packing.
  - Paper and Corrugation Packing.
  - Engineering Products Packing.
  - Bottle and Can Packing
  - Appliance Packing.

- ### Full Specifications of Pet Strapping

  S.No. | Strap Code | Reference | Width (in mm) | Thickness (in mm) | Type | Roll Length (in mtrs.) | Break Strength (in kgf) | Elongation (in %)
  --- | --- | --- | --- | --- | --- | --- | --- | ---
  1 | 095060E | 09.5 x 0.60 | 9.5 +/- 0.6 | 0.60 +/- 0.05 | Emboss | 3000 | 200 +/- 10 | 10 - 16%
  2 | 095080E | 09.5 x 0.80 | 9.5 +/- 0.6 | 0.60 +/- 0.05 | Emboss | 2500 | 290 +/- 15 | 10 - 16%
  3 | 110060S | 11.0 x 0.60 | 11.0 +/- 0.6 | 0.60 +/- 0.05 | Smooth | 3000 | 290 +/- 10 | 10 - 16%
  4 | 110070E | 11.0 x 0.70 | 11.0 +/- 0.6 | 0.70 +/- 0.05 | Emboss | 3000 | 290 +/- 15 | 10 - 16%
  5 | 120050E | 12.0 x 0.50 | 12.0 +/- 0.6 | 0.50 +/- 0.05 | Emboss | 3000 | 210 +/- 10 | 10 - 16%
  6 | 120060E | 12.0 x 0.60 | 12.0 +/- 0.6 | 0.60 +/- 0.05 | Emboss | 2600 | 260 +/- 20 | 10 - 16%
  7 | 120070E | 12.0 x 0.70 | 12.0 +/- 0.6 | 0.70 +/- 0.05 | Emboss | 2600 | 300 +/- 15 | 10 - 16%
  8 | 120080E | 12.0 x 0.80 | 12.0 +/- 0.6 | 0.80 +/- 0.05 | Emboss | 2600 | 370 +/- 15 | 10 - 16%
  9 | 120090S | 12.0 x 0.90 | 12.0 +/- 0.6 | 0.90 +/- 0.05 | Smooth | 2000 | 470 +/- 20 | 10 - 16%
  10 | 140070S | 14.0 x 0.70 | 14.0 +/- 0.6 | 0.70 +/- 0.05 | Smooth | 1725 | 430 +/- 20 | 10 - 16%
  11 | 150060S | 15.0 x 0.60 | 15.0 +/- 0.6 | 0.60 +/- 0.05 | Smooth | 1500 | 390 +/- 15 | 10 - 16%
  12 | 150060E | 15.0 x 0.60 | 15.0 +/- 0.6 | 0.60 +/- 0.05 | Emboss | 2400 | 340 +/- 15 | 10 - 16%
  13 | 150070E | 15.0 x 0.70 | 15.0 +/- 0.6 | 0.70 +/- 0.05 | Emboss | 1600 | 390 +/- 20 | 10 - 16%
  14 | 155076S | 15.5 x 0.76 | 15.5 +/- 0.6 | 0.76 +/- 0.05 | Smooth | 1250 | 510 +/- 25 | 10 - 16%
  15 | 155080S | 15.5 x 0.80 | 15.5 +/- 0.6 | 0.80 +/- 0.05 | Smooth | 1250 | 540 +/- 25 | 10 - 16%
  16 | 155090S | 15.5 x 0.90 | 15.5 +/- 0.6 | 0.90 +/- 0.05 | Smooth | 1250 | 610 +/- 20 | 10 - 16%
  17 | 155100S | 15.5 x 1.00 | 15.5 +/- 0.6 | 1.00 +/- 0.05 | Smooth | 1100 | 680 +/- 30 | 10 - 16%
  18 | 160070E | 16.0 x 0.70 | 16.0 +/- 0.6 | 0.70 +/- 0.05 | Emboss | 1600 | 420 +/- 20 | 10 - 16%
  19 | 160080S | 16.0 x 0.80 | 16.0 +/- 0.6 | 0.80 +/- 0.05 | Smooth | 1250 | 560 +/- 25 | 10 - 16%
  20 | 160088S | 16.0 x 0.88 | 16.0 +/- 0.6 | 0.88 +/- 0.05 | Smooth | 1250 | 620 +/- 30 | 10 - 16%
  21 | 160090S | 16.0 x 0.90 | 16.0 +/- 0.6 | 0.90 +/- 0.05 | Smooth | 1100 | 630 +/- 25 | 10 - 16%
  22 | 160100S | 16.0 x 1.00 | 16.0 +/- 0.6 | 1.00 +/- 0.05 | Smooth | 1100 | 700 +/- 30 | 10 - 16%
  23 | 190070S | 19.0 x 0.70 | 19.0 +/- 0.6 | 0.70 +/- 0.05 | Smooth | 1000 | 580 +/- 25 | 10 - 16%
  24 | 190080S | 19.0 x 0.80 | 19.0 +/- 0.6 | 0.80 +/- 0.05 | Smooth | 1000 | 660 +/- 30 | 10 - 16%
  25 | 190090S | 19.0 x 0.90 | 19.0 +/- 0.6 | 0.90 +/- 0.05 | Smooth | 1000 | 750 +/- 30 | 10 - 16%
  26 | 190100S | 19.0 x 1.00 | 19.0 +/- 0.6 | 1.00 +/- 0.05 | Smooth | 1000 | 830 +/- 40 | 10 - 16%
  27 | 190127S | 19.0 x 1.27 | 19.0 +/- 0.6 | 1.27 +/- 0.05 | Smooth | 730 | 1060 +/- 50 | 10 - 16%
  28 | 250100S | 25.0 x 1.00 | 25.0 +/- 0.6 | 1.00 +/- 0.05 | Smooth | 650 | 1100 +/- 50 | 10 - 16%

- ### contact address

  Office : U/L 24, Pattani Plaza, Devbaug Road,
  Bhavnagar-364001, Gujarat, India.
  Telephone : +91 278 2438266, +91 278 2438113.
  Fax : +91 278 2438280.
  Mobile : +91 98250 94923.
  E-mail : nagin@strapsindia.com, info@strapsindia.com
  Website : www.strapsindia.com, www.sujlonropes.com, www.surajfilaments.com.

  ### contact form

- ### Pet Strapping

  Straps India is having world best twin screw extrusion line from Reimotec gmbh Germany for pet strap production. Due to latest technology company guarantees best strength in Pet Straps.

  Pet Strapping is available in smooth, plain and emboss knurling surface. All pet straps manufactured by our company is 100% suitable for fully automatic machines applications. We offer min size variation in all our pet straps in industry.

  Pet Strap is available from 9mm to 25mm width. And thickness from 0.50mm to 1.27mm. Pet Strap is available in green, black and white color.

  Printed strap with logo is available on request.

  ### Company provides pet strapping for following industries

  - Cotton Baling.
  - Fibre Baling.
  - Poly Packet Packing.
  - Tiles & Paver Block Packing.
  - Timber & Wood Packing.
  - Alluminium Ingot Packing.
  - All Kind Of Film Packing.
  - Glass Packing.
  - Paper and Corrugation Packing.
  - Engineering Products Packing.
  - Bottle and Can Packing
  - Appliance Packing.

- ### Pet Strapping Tools

  Company provides full range of pneumatic and battery operated pet strapping tools made by M J Maillis. Full specs for all kind of tools are readily available.

  We are also providing on site contract packing for all industries. We also deals in all kind of tool maintenance jobs, AMC for tools, preventies maintenance of pet strapping tools.

- ### PP Multi Filaments Yarn

  Company provides high tenacity PP multi filament yarn produced with world best extrusion line of SML Austria. We are offering high tenacity PP multi filament yarn from 210D 5000D in flat, intermingled, twisted construction.

  All high tenacity PP multi filament yarn is available in UV and various colors as per customer requirements.

  ### Company supplies PP multi filament yarn for following applications

  - Filter fabrics and industrial fabrics.
  - Geo textile.
  - HDPE and PP woven sack industries for mouth and bottom stitching of bags.
  - Use in Fibc for stitching and webbing.
  - Shoe stitching.
  - PVC hose pipe reinforcement.
  - High tenacity slings.
  - Narrow woven fabrics and webbing industry.
  - PP mat industry(CHATAI).

- ### PP Crimp Yarn

  Company owns JSW extrusion line with TEIJIN SEIKI winders for production of PP crimping yarn, PP crimp yarn is available from 65D to 520D in all colors. We offer PP crimp yarn with 2% uv (food grade) for jumbo bag application.

  PP Crimp Yarn is used mainly for socks, hosiery, knitting items and filler cord.

  We also offer PP filler cord which is used for dust proofing of all kind of FIBC (Jumbo Bags). Filler cord is also available with 2% uv on customer request.

- ### High Tenacity Twine

  We MFR all types of two and multiple plied twine commonly used as stitching and sewing thread for bags in sugar, rice and fertilizer industry.

  Apart from these applications our high tenacity twine is also used for mfr of all kind of fishing nets, agricultural nets and safety nets. High tenacity twine is available in white, blue and green color.

  - 210D 3 x 2.
  - 210D 4 x 2.
  - 500D 1 x 2.
  - 600D 1 x 2.
  - 730D 1 x 2.
  - 840D 1 x 2.
  - 840D 1 x 3.
  - 840D 2 x 3.
  - 840D 3 x 3.

- ### PP Ropes

  We are having Korean extrusion line for production of PP Danline Ropes. We offer PP Danline Ropes from 1.50mm to 36mm thickness in three and four stand.

  PP Danline Rope is available in yellow, green and white color. We also offer PP Danline Ropes with uv.

  ### PP Danline Rope is used mainly for

  - Fishing.
  - Shipping and Mooring.
  - Ports and Ship Building.
  - Stevedoring.
  - Defense.
  - Material Handling.
  - Construction.
  - Industrial Applications.